8-1 续表 |  |  |  | continued |  |  |  |  |  |  |  |  |  |  |  |
指标名称 | Item | 2000 | 2002 | 2003 | 2004 |
市政设施 | Municipal Engineering |  |
道路长度(公里) | Length of Paved Roads (km) | 4739 | 4978.57 | 5368.9 | 5539.89 |
道路面积(万平方米) | Area of Paved Roads (10 000 sq.m) | 4815.93 | 6900.4 | 7980.8 | 8788.1 |
人行道面积(万平方米) | Area of Sidewalk (10 000 sq.m) | 1426.82 | 1810.5 | 1892.5 | 2012.5 |
桥梁数(座) | Number of bridges (unit) | 637 | 538 | 541 | 504 |
#立交桥 | #Cloverleaf Junction | 82 | 72 | 74 | 62 |
路灯(盏) | Number of Street Lights (unit) | 115147 | 178122 | 224858 | 255498 |
排水管道长度(公里) | Length of Sewer Pipelines (km) | 3754.31 | 4089.54 | 4404.02 | 4946.36 |
污水排放量(万立方米) | Number Volume of Let Sewage (10 000 cu.m) | 165902 | 139159 | 150235 | 162878 |
污水处理厂(座数) | Number of Sewage Disposal Farm (unit) | 21 | 13 | 13 | 15 |
处理能力(万立方米/日) | Daily Disposal Capacity of Sewage (10 000 cu.m/day) | 61.15 | 64.4 | 73.4 | 117.4 |
设施能力(万立方米/日) | Capacity of Engineering (10 000 cu.m/day) | 83.9 | 103.49 | 149.64 | 211.04 |
污水年处理量(万立方米) | Annual Volume of Sewage Treated (10 000 cu.m) | 45316 | 26340.5 | 40285 | 62109.4 |
防洪堤长度(公里) | Length of Banks to Prevent or Control Flood (km) | 602.77 | 541.5 | 761.27 | 846.91 |
#百年一遇以上 | # Befall 100 Years and Over | 107.03 | 49.9 | 21.7 | 113.2 |
人均拥有道路(平方米) | Per Capita of Road Areas (sq.m) | 6.96 | 6.56 | 7.9 | 8.69 |
排水管密度(公里／平方公里) | Density of Drainage Pipelines (km/sq.km) | 4.7 | 4.56 | 4.59 | 4.93 |
污水处理率(%) | Rate of Sewage Disposal (%) | 27.31 | 18.93 | 26.81 | 38.13 |
园林绿化 | Parks, Gardens and Green Areas |  |  |  |
绿化覆盖面积(公顷) | Coverage Space of Green Areas (hectare) | 49290 | 37760.1 | 39544.9 | 42224.8 |
#建成区 | #Developed Area | 22646 | 25671.3 | 28827 | 32250.4 |
园林绿地面积(公顷) | Area of Parks,Gardens and Green Areas in Cities (hectare) | 44672 | 31825.5 | 34254.8 | 36107.3 |
#建成区 | #Developed Area | 19450 | 22434.3 | 25050.8 | 26661.7 |
公共绿地面积(公顷) | Public Green Areas (hectare) | 3525 | 4970.26 | 5116.29 | 6605.11 |
公园个数(个） | Number of Parks (unit) | 116 | 122 | 129 | 149 |
公园面积(公顷) | Area of Parks (hectare) | 2646.41 | 3222.86 | 3513.39 | 5038.13 |
人均公共绿地面积(平方米) | Per Capita Public Green Areas (sq.m) | 5.1 | 4.72 | 5.07 | 6.53 |
建成区绿地率(%) | Rate of Green Areas Developed (%) | 24.33 | 24.99 | 26.11 | 26.59 |
建成区绿化覆盖率(%) | Coverage Rate of Green Areas Developed (%) | 28.33 | 28.6 | 30.05 | 32.16 |
环境卫生 | Environmental Sanitation |  |  |  |
实际清扫面积(万平方米) | Area Under Cleaning Program (10 000 sq.m) | 3236.22 | 4627.7 | 5402.1 | 6690 |
#机械清扫 | Machine Cleaning | 411.77 | 656.3 | 814.6 | 1076.3 |
生活垃圾清运量(万吨) | Volume of Garbage Disposal (10 000 tons) | 358.46 | 459 | 444 | 489 |
粪便清运量(万吨) | Volume of Excrement and Urine Disposal (10 000 tons) | 24.25 | 50.3 | 64.1 | 66.5 |
垃圾无害化处理场(座数) | Number of Factories to Treat Garbage Harmlessly(unit) | 15 | 26 | 2 | 6 |
#处理能力(吨/日) | Daily Disposal Capacity (ton/day) | 4427 | 7736 | 2762 | 5603 |
垃圾无害处理量(万吨) | Volume of Garbage Harmlessly Treatment (10 000 tons) | 180.91 | 252.22 | 100 | 159 |
粪便无害化处理量(万吨) | Volume of Urine Harmlessly Treatment (10 000 tons) | 8.31 | 48.2 | 61.2 | 61.1 |
公共厕所数(座) | Number of Public Lavatories (unit) | 3001 | 2465 | 2538 | 2728 |
#水冲式 | # Water Closet | 1771 | 1822 | 1919 | 2250 |
环卫机械总数(台) | Environmental Sanitation Equipment (unit) | 1213 | 1012 | 867 | 1136 |
年末环卫工人数(人) | Environmental Sanitation Workers at Year-end (person) | 11356 | 19885 | 19300 | 20129 |
生活垃圾无害化处理率(%) | Ratio of Garbage Harmlessly Treatment (%) | 50.47 | 54.9 | 24.17 | 32.52 |
粪便处理率(%) | Ratio of Urine Harmlessly Treatment (%) | 34.27 | 95.83 | 92.49 | 91.88 |
194 |