6-1 续表 continued |  |  |  |  |  |  |  |  |  |  |  |
指标名称 | Item | 2000 | 2004 | 2005 | 2006 |
市政设施 | Municipal Engineering |  |
道路长度(公里) | Length of Paved Roads (km) | 4739 | 5539.89 | 5978.24 | 6577 |
道路面积(万平方米) | Area of Paved Roads (10 000 sq.m) | 4815.93 | 8788.1 | 9935.8 | 11063 |
人行道面积(万平方米) | Area of Sidewalk (10 000 sq.m) | 1426.82 | 2012.5 | 2411 | 2472 |
桥梁数(座) | Number of bridges (unit) | 637 | 504 | 482 | 483 |
#立交桥 | #Cloverleaf Junction | 82 | 62 | 48 | 62 |
路灯(盏) | Number of Street Lights (unit) | 115147 | 255498 | 295972 | 318000 |
排水管道长度(公里) | Length of Sewer Pipelines (km) | 3754.31 | 4946.36 | 5593.83 | 6638 |
污水排放量(万立方米) | Number Volume of Let Sewage (10 000 cu.m) | 165902 | 162878 | 169530 | 177867 |
污水处理厂(座数) | Number of Sewage Disposal Farm (unit) | 21 | 15 | 19 | 20 |
处理能力(万立方米/日) | Daily Disposal Capacity of Sewage (10 000 cu.m/day) | 61.15 | 117.4 | 135.4 | 136.4 |
设施能力(万立方米/日) | Capacity of Engineering (10 000 cu.m/day) | 83.9 | 211.04 | 152.27 | 346.3 |
污水年处理量(万立方米) | Annual Volume of Sewage Treated (10 000 cu.m) | 45316 | 62109.4 | 68739.7 | 75988 |
防洪堤长度(公里) | Length of Banks to Prevent or Control Flood (km) | 602.77 | 846.91 | 1119.15 | 1082 |
#百年一遇以上 | # Befall 100 Years and Over | 107.03 | 113.2 | 272.53 | 174 |
人均拥有道路(平方米) | Per Capita of Road Areas (sq.m) | 6.96 | 8.69 | 9.56 | 10.68 |
排水管密度(公里／平方公里) | Density of Drainage Pipelines (km/sq.km) | 4.7 | 4.93 | 5.42 | 1.9 |
污水处理率(%) | Rate of Sewage Disposal (%) | 27.31 | 38.13 | 40.55 | 42.72 |
园林绿化 | Parks, Gardens and Green Areas |  |
绿化覆盖面积(公顷) | Coverage Space of Green Areas (hectare) | 49290 | 42224.8 | 44642.5 | 42943 |
#建成区 | #Developed Area | 22646 | 32250.4 | 34175.5 | 36025 |
园林绿地面积(公顷) | Area of Parks,Gardens and Green Areas in Cities (hectare) | 44672 | 36107.3 | 40723.3 | 35314 |
#建成区 | #Developed Area | 19450 | 26661.7 | 30506 | 32620 |
公共绿地面积(公顷) | Public Green Areas (hectare) | 3525 | 6605.11 | 7143.2 | 7722 |
公园个数(个） | Number of Parks (unit) | 116 | 149 | 150 | 154 |
公园面积(公顷) | Area of Parks (hectare) | 2646.41 | 5038.13 | 6589.31 | 5135 |
人均公共绿地面积(平方米) | Per Capita Public Green Areas (sq.m) | 5.1 | 6.53 | 6.87 | 6.99 |
建成区绿地率(%) | Rate of Green Areas Developed (%) | 24.33 | 26.59 | 29.53 | 31.46 |
建成区绿化覆盖率(%) | Coverage Rate of Green Areas Developed (%) | 28.33 | 32.16 | 33.09 | 34.74 |
环境卫生 | Environmental Sanitation |  |
实际清扫面积(万平方米) | Area Under Cleaning Program (10 000 sq.m) | 3236.22 | 6690 | 7559.7 | 9378 |
#机械清扫 | Machine Cleaning | 411.77 | 1076.3 | 1148.7 | 1559 |
生活垃圾清运量(万吨) | Volume of Garbage Disposal (10 000 tons) | 358.46 | 489 | 486 | 510 |
粪便清运量(万吨) | Volume of Excrement and Urine Disposal (10 000 tons) | 24.25 | 66.5 | 41.4 | 40 |
垃圾无害化处理场(座数) | Number of Factories to Treat Garbage Harmlessly(unit) | 15 | 6 | 7 | 8 |
#处理能力(吨/日) | Daily Disposal Capacity (ton/day) | 4427 | 5603 | 6122 | 6030 |
垃圾无害处理量(万吨) | Volume of Garbage Harmlessly Treatment (10 000 tons) | 180.91 | 159 | 192.9 | 236.3 |
粪便无害化处理量(万吨) | Volume of Urine Harmlessly Treatment (10 000 tons) | 8.31 | 61.1 | 40.2 | 31.7 |
公共厕所数(座) | Number of Public Lavatories (unit) | 3001 | 2728 | 2652 | 2597 |
#水冲式 | # Water Closet | 1771 | 2250 | 2240 | 1781 |
环卫机械总数(台) | Environmental Sanitation Equipment (unit) | 1213 | 1136 | 1396 | 1342 |
年末环卫工人数(人) | Environmental Sanitation Workers at Year-end (person) | 11356 | 20129 | 24500 | 24518 |
生活垃圾无害化处理率(%) | Ratio of Garbage Harmlessly Treatment (%) | 50.47 | 32.52 | 39.69 | 46.3 |
172 |