6-1 续表 continued |  |  |  |  |  |  |  |  |  |  |  |
指标名称 | Item | 2000 | 2005 | 2006 | 2007 |
市政设施 | Municipal Engineering |  |
道路长度(公里) | Length of Paved Roads (km) | 4739 | 5978 | 6577 | 7144 |
道路面积(万平方米) | Area of Paved Roads (10 000 sq.m) | 4815.9 | 9935.8 | 11063.0 | 12740.0 |
人行道面积(万平方米) | Area of Sidewalk (10 000 sq.m) | 1426.8 | 2411.0 | 2472.0 | 3127.0 |
桥梁数(座) | Number of bridges (unit) | 637 | 482 | 483 | 505 |
#立交桥 | #Cloverleaf Junction | 82 | 48 | 62 | 63 |
路灯(盏) | Number of Street Lights (unit) | 115147 | 295972 | 318000 | 319000 |
排水管道长度(公里) | Length of Sewer Pipelines (km) | 3754 | 5594 | 6638 | 7610 |
污水排放量(万立方米) | Number Volume of Let Sewage (10 000 cu.m) | 165902 | 169530 | 177867 | 154783 |
污水处理厂(座数) | Number of Sewage Disposal Farm (unit) | 21 | 19 | 20 | 26 |
处理能力(万立方米/日) | Daily Disposal Capacity of Sewage (10 000 cu.m/day) | 61.2 | 135.4 | 136.4 | 220.4 |
设施能力(万立方米/日) | Capacity of Engineering (10 000 cu.m/day) | 83.9 | 152.3 | 346.3 |  |
污水年处理量(万立方米) | Annual Volume of Sewage Treated (10 000 cu.m) | 45316.0 | 68739.7 | 75988.0 | 71731.0 |
防洪堤长度(公里) | Length of Banks to Prevent or Control Flood (km) | 603 | 1119 | 1082 | 1990 |
#百年一遇以上 | # Befall 100 Years and Over | 107 | 273 | 174 | 208 |
人均拥有道路(平方米) | Per Capita of Road Areas (sq.m) | 7.0 | 9.6 | 10.7 | 11.4 |
排水管密度(公里／平方公里) | Density of Drainage Pipelines (km/sq.km) | 4.7 | 5.4 | 1.9 | 2.6 |
污水处理率(%) | Rate of Sewage Disposal (%) | 27.3 | 40.6 | 42.7 | 46.3 |
园林绿化 | Parks, Gardens and Green Areas |  |
绿化覆盖面积(公顷) | Coverage Space of Green Areas (hectare) | 49290 | 44643 | 42943 | 47487 |
#建成区 | #Developed Area | 22646 | 34176 | 36025 | 39560 |
园林绿地面积(公顷) | Area of Parks,Gardens and Green Areas in Cities (hectare) | 44672 | 40723 | 35314 | 39742 |
#建成区 | #Developed Area | 19450 | 30506 | 32620 | 35685 |
公共绿地面积(公顷) | Public Green Areas (hectare) | 3525 | 7143 | 7722 | 8520 |
公园个数(个） | Number of Parks (unit) | 116 | 150 | 154 | 159 |
公园面积(公顷) | Area of Parks (hectare) | 2646 | 6589 | 5135 | 5545 |
人均公共绿地面积(平方米) | Per Capita Public Green Areas (sq.m) | 5.1 | 6.9 | 7.0 | 7.6 |
建成区绿地率(%) | Rate of Green Areas Developed (%) | 24.3 | 29.5 | 31.5 | 32.1 |
建成区绿化覆盖率(%) | Coverage Rate of Green Areas Developed (%) | 28.3 | 33.1 | 34.7 | 35.6 |
环境卫生 | Environmental Sanitation |  |
实际清扫面积(万平方米) | Area Under Cleaning Program (10 000 sq.m) | 3236.2 | 7559.7 | 9378.0 | 10052.0 |
#机械清扫 | Machine Cleaning | 411.8 | 1148.7 | 1559.0 | 4740.0 |
生活垃圾清运量(万吨) | Volume of Garbage Disposal (10 000 tons) | 358.46 | 486.00 | 510.00 | 511.17 |
粪便清运量(万吨) | Volume of Excrement and Urine Disposal (10 000 tons) | 24.25 | 41.40 | 40.00 | 38.30 |
垃圾无害化处理场(座数) | Number of Factories to Treat Garbage Harmlessly(unit) | 15 | 7 | 8 | 14 |
#处理能力(吨/日) | Daily Disposal Capacity (ton/day) | 4427 | 6122 | 6030 | 8650 |
垃圾无害处理量(万吨) | Volume of Garbage Harmlessly Treatment (10 000 tons) | 180.91 | 192.90 | 236.30 | 269.73 |
粪便无害化处理量(万吨) | Volume of Urine Harmlessly Treatment (10 000 tons) | 8.31 | 40.20 | 31.70 | 0.02 |
公共厕所数(座) | Number of Public Lavatories (unit) | 3001 | 2652 | 2597 | 2714 |
#水冲式 | # Water Closet | 1771 | 2240 | 1781 | 1754 |
环卫机械总数(台) | Environmental Sanitation Equipment (unit) | 1213 | 1396 | 1342 | 1486 |
年末环卫工人数(人) | Environmental Sanitation Workers at Year-end (person) | 11356 | 24500 | 24518 |  |
生活垃圾无害化处理率(%) | Ratio of Garbage Harmlessly Treatment (%) | 50.5 | 39.7 | 46.3 | 52.8 |
182 |