9-11 主要用能工业企业单位产品能源消耗情况
Unit Product Energy Consumption of Industry
千克标准煤/吨 |  | (kg of SCE / ton)
指标 | Item | 2007 | 2008
吨原煤生产综合能耗(千瓦时/吨） | Total Energy Consumption of Raw Coal/ton | 144.43 | 137.56
万米印染布综合能耗(千克标准煤/万米) | Total Energy Consumption of Dyed Cloth/10,000m | 2039.47 | 2016.72
机制纸及纸板综合能耗(千瓦时/吨） | Total Energy Consumption of Machine-Made Paper and Paperboard | 631.72 | 635.22
炼焦工序单位能耗 | Energy Consumption of Coking Process/unit | 152.20 | 140.14
原油加工单位综合能耗 | Total Energy Consumption of Crude Oil Processing/unit | 71.94 | 69.63
单位烧碱生产综合能耗(离子膜法30%） | Total Energy Consumption of Caustic Soda Production/unitunit (Ion-exchange Membrane Process 30%) | 648.55 | 644.40
单位烧碱生产综合能耗(隔膜法30%） | Total Energy Consumption of Caustic Soda Production/unit (Diaphragm Process 30%) | 610.93 | 590.45
单位烧碱生产综合能耗(隔膜法96%） | Total Energy Consumption of Caustic Soda Production/unit (Diaphram Process 96%) | 771.15 | 768.93
氨碱法单位纯碱生产综合能耗 | Total Energy Consumption of Soda Production/unit (ammonia-soda process) | 297.09 | 282.00
联碱法纯碱双吨产品生产综合能耗 | Total Energy Consumption of Soda Production/double tons (Hou's process) | 185.73 | 200.72
单位合成氨生产综合能耗 | Total Energy Consumption of Synthetic Ammonia/unit | 1300.88 | 1287.80
吨水泥熟料综合能耗 | Total Energy Consumption of Cement/ton | 146.38 | 142.81
吨水泥综合能耗 | Total Energy Consumption of Cement Per Ton | 119.94 | 115.46
每重量箱平板玻璃综合能耗(千克标准煤/重量箱) | Total Energy Consumption of Plate Glass/weight box | 15.33 | 14.94
吨钢综合能耗 | Total Energy Consumption of Steel/ton | 636.82 | 623.47
炼铁工序单位能耗 | Unit Energy Consumption of Iron Refining Process | 421.85 | 417.03
铁矿烧结工序单位能耗 | Unit Energy Consumption of Iron Ore Sintering Process | 54.10 | 54.51
转炉炼钢综合工序单位能耗 | Unit Energy Consumption of Converter Steelmaking Process | 14.99 | 13.74
电炉炼钢综合工序单位能耗 | Unit Energy Consumption of Electric Furnace Steelmaking Process | 135.78 | 126.71
硅锰合金工序单位能耗（千克标准煤/标准吨） | Unit Energy Consumption of Silicomanganese Alloy Process | 1445.64 | 1365.99
轧钢工序单位能耗 | Unit Energy Consumption of Steel Rolling Process | 72.45 | 72.14
吨钢耗新水（吨/吨） | New Water Consumption of Steel/ton | 8.08 | 7.27
单位铜冶炼综合能耗 | Total Energy Consumption of Copper Refining/unit | 485.68 | 462.48
单位氧化铝综合能耗 | Total Energy Consumption of Alumina/unit | 780.40 | 769.28
单位粗铅综合能耗 | Total Energy Consumption of Crude Lead/unit | 309.50 | 308.02
单位铅冶炼综合能耗 | Total Energy Consumption of Lead Refining/unit | 496.31 | 490.99
蒸镏锌综合标准煤耗单耗 | Standard Coal Consumption of Distillated Zinc | 1536.40 | 1535.93
单位精锌（电锌）综合能耗 | Total Consumption of Refined Zinc(Electrolytic Zinc)/unit | 1084.80 | 1022.60
吨铝加工材消耗能源量 | Energy Consumption of Aluminium Processing Material/ton | 796.87 | 783.03
电厂火力发电标准煤耗(克标准煤/千瓦时) | Standard Coal Consumption of Thermal Power Generation in the Power Plant | 318.27 | 318.39
电厂火力供电标准煤耗(克标准煤/千瓦时) | Standard Coal Consumption of Thermal Power Supply in the Power Plant | 343.98 | 341.40
270